**SECTION 01500**

**DELIVERY, STORAGE, & HANDLING**

1. **GENERAL**
   1. **WORK INCLUDED**
      1. Products to be used in the Work shall be properly stored and handled as described in this section, but not necessarily limited to them.
   2. **RELATED WORK**
      1. Additional procedures may also be prescribed in other sections of these Specifications.
   3. **QUALITY ASSURANCE**
      1. The Contractor shall ensure that the necessary measures be taken to protect the materials and work as required.
   4. **MANUFACTURER’S RECOMMENDATION**
      1. Unless otherwise approved by the Engineer or specified herein, the Contractor shall comply with the manufacturer’s recommendations on product handling. Storage and protection.
   5. **PACKAGING**
      1. Products shall be delivered to the job site in their manufacturer’s original container with labels intact and legible. All equipment shall have the manufacturer’s serial number plates. Damaged materials shall be immediately replaced at no additional cost to the owner. The Engineer may reject, as non-complying, any materials that do not beat the proper identification such as manufacturer, grade, quality, and other pertinent information.
   6. **PROTECTION**
      1. The contractor shall protect and maintain all finished surfaces, the Contractor shall make the necessary replacements and repairs to the approval of the Engineer at no additional cost to the Owner. No extension of contract time will be given for work associated with replacement and repair of damaged materials and work.
   7. **DELIVERY & STORAGE**
      1. Delivery: The Contractor shall be responsible for making all the arrangements for the delivery, unloading, receiving and storage of materials. The Owner will not be responsible for these duties.
      2. Storage: The Contractor shall store all products and materials in a protected location to prevent any damage or deterioration due to moisture, freezing temperatures or other detrimental conditions.
   8. **DAMAGED OR REJECTED MATERIAL**
      1. Any damaged or rejected material shall be removed from the job site immediately.
2. **PRODUCTS – NOT USED**
3. **EXECUTION – NOT USED**

END SECTION